4.12.01 - 03/13/2023 12:37:00 PM
  - Initial release  
  
4.12.02 - 05/08/2023 3:20:20 PM
  - All "Refresh log" links moved to top of page
  
4.12.03 - 05/13/2023 3:17:41 PM
  - Router4.4.29
    - fclose if config fails   
    
4.12.04 - 05/31/2023 11:44:39 AM
  - DH+ Monitor shows changes
  - Logs 
    - scroll to bottom initially and on refresh
    - Auto Refresh

4.12.05 - 06/28/2023 5:33:52 PM
  - Turn off 'Auto Refresh' if Previous log is chosen     
  
4.12.06 - 07/24/2023 11:26:14 AM     
  - corrected H1 size in anxstyle.css

4.12.07 - 2024-02-12 17:00:50
  - DHP PRU RxMsg did not mask RxAck, did not recognize 0x88 as valid ACK
  
4.14.01 - 2024-02-15 18:37:10
  - Long DHP messages were not processed correctly by MsgRouter
    - MsgCtl->CipLength changed to WORD

4.14.02 - 2024-03-13 10:49:06
  - 230k gap time from 15 to 20
  
4.15.03 - 2024-04-08 17:50:27
  - Added Modbus TCP server
  - AN-X-DHP Home link identifies firmware
  - Web page Titles match Left Menu
  - Clarified text on home page
  - Clarified text on many other pages
  - Web pages left aligned for consistent look on different browser widths
  
4.15.04 -  2024-04-09
  - Added Modbus TCP max connections to sample config
  
4.15.05 - 2024-05-08
  - Modbus TCP SLC mappings use Fnc aa & a2
    - bug fixes and improved sample  

4.15.06 - 2024-05-28 09:39:56
  - Modbus TCP allow SLC I & O file write
  
4.16.02 - 2025-09-18
  - Added CIP Data Table Read/Write support
    - PLC-5 and SLC

4.16.03 - 2025-10-24
	- CIP Data Table Read/Write
	  - translate N7_100 to N7:100